PLD Do’s and Do not’s

1. Do not allow the turbo pump to reach atmospheric pressure when it is running.
2. Do close the gate valve before venting the chamber.
3. Do open the door latch when venting the chamber.
4. Do only put approved materials in the chamber.
5. Do not fire the laser without a target in holder.
6. Do put down heater when ablating.
7. Do not ever allow the laser to vent to atmosphere.
8. Do not clean the window with any grit above 1µm.
9. Do clean up after yourself.